Q: When UE performing DRX operation in sleeping state, the RNC buffers newly arrived packets without transmissions until UE wakes up and receive buffered packets. Why we can use M/G/1 queuing model to describe the packet transmission delay? And using Pollaczek-Khinchine formula to present packet transmission delay () in immediate-transmitting state.